CONSOLE COIN/CUP HOLDER BINDS (DIAGNOSTIC PROCEDURE). Oldsmobile Toronado 1988

For 1990-2009 cars

# CONSOLE COIN/CUP HOLDER BINDS (DIAGNOSTIC PROCEDURE)

1986-1989 E

Some 1986-1989 Toronado vehicles equipped with a centre console may experience a condition where the coin/cup holder binds or requires excessive effort to operate. This condition may be caused by any of the following:

Interference of the coin/cup holder with console wiring. Distorted coin/cup mounting plate. Defective coin/cup mounting plate.

To repair this condition use the following procedure:

1. Remove console trim plate. 2. Remove shift indicator assembly. 3. Remove coin/cup mounting plate assembly. 4. Refer to trouble tree on next page.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.