INT./EXT. PAINT CODES- MOLDINGS AND STRIPING COLORS. Oldsmobile Toronado 1983

For 1990-2009 cars

# INT./EXT. PAINT CODES- MOLDINGS AND STRIPING COLORS

The three production paint suppliers (Ditzler, DuPont and Rinshed-Mason), now have 1983 service paint in their Field Warehouses or Regional Distributorships. The paints listed in this bulletin will be available from local paint suppliers in the near future.

#### NOTE: Service paint is also available from paint refinish specialists such as Sherwin-Williams, Acme, Rogers, and Martin-Senour. Paint suppliers in your area can provide you with information regarding these materials.

When contacting your local paint supplier for repair materials, make sure that you specify the type of material needed. If your paint supplier is unable to provide you with the material needed, ask him to contact his manufacturer sales representative for assistance.

EXTERIOR COLORS Sherwin- Paint Inmont Williams Martin- Code Color Name Ditzler Dupont (R.M.) (Acme/Rogers) Senour ---- ---------- ------- ------ ------ ------------- ------ 11 White 2058 5338 2080 L10A-2864 30-3929 5644 15 Silver Sand Met. 3520 B8302 13100 33188 30-5256 19 Black 9300 99 A946 L10B-1738 3069 3000-4590 22 Lt. Royal Blue Met. 3522 B8308 13106 32895 30-5229 77 Med. Dk. Royal Blue Met. 3525 B8304 13110 32701 30-5179 42 Lt. Gray Fern Met. 3526 B8309 13114 32902 30-5234 48 Dk. Gray Fern Met. 3528 B8303 13115 32702 30-5180 52 Lt. Beech Met N/A N/A 13520 33481 30-5264 59 Cream Beige 3087 45205 13521 33479 30-5262 60 Lt. Sand Gray 3530 B8307 13120 32704 30-5182 62 Lt. Briar Brown Met. 3531 B8310 13121 32896 30-5230 67 Dk. Briar Brown Met. 3533 B8305 13127 32705 30-5183 73 Lt. Maple Met. 3331 B8108 13522 33480 30-5263 74 Autumn Maple F/M 3532 B8385 13131 33074 30-5244 75 Spectra Red 3332 B8115 12229 31056 30-4989 78 Dk. Autumn Maple Met. 3553 B8306 13132 33075 30-5245 87 Med. Sand Gray F/M 3538 B8311 13135 32706 30-5184 91 Lt. Flax F/M 3540 C8303 13137 33240 30-5259

INTERIOR COLORS

#### NOTICE: Ditzler DIA is Duracryl Interior Lacquer, Ditzler UCV is Liquid Vinyl Paint for Vinyl and ABS plastic parts (instrument panels, door trim panels, seats, etc.) DuPont is Interior Lacquw. Rinshed-Mason is Interior Lacquer. Sherwin-Williams is interior Lacquer. When painting interior flexible parts, add R-M 891 flex agent.

Sherwin- Code Ditzler Ditzler Inmont Williams Martin/ Semi-Gloss Color Name DIA UCV Dupont (R.M.) Acme/Rogers Senour ---------- ---------- --- --- ------ ---- ----------- ------ 17 Med. Dk. Charcoal 33569 2.1034 C8339 13195 32841 32-17020 17 Dark Charcoal 33570 2.976 C8387 31394 32842 32-17021 19 Black 9387 120 4428 4401 J4-3960 32-16082 90681 22 Med. Dk. Royal Blue 15680 2.1033 C8334 13192 32999 32-16915 22 Dark Royal Blue 15632 2.974 C8336 13191 32839 32-17018 42 Med. Grayfern 33586 2.975 C8336 13187 32840 32-17019 42 Dark Grayfern 33687 2.971 C8327 13186 32836 32-17015 60 Lt.Sand Gray 33567 2,972 C8384 13182 32837 32-17016 60 Med.Sand Gray 33568 2.973 C8329 13181 32838 32-17017 61 Med.Saddle Tan 24997 2.878 D8208 12139 31892 32-16842 61 Dark Saddle Tan 24999 2.880 D8217 12741 31893 32-16843 67 Med. Dk. Briar Brown 25306 2.1043 C8340 13176 33283 32-16845 67 Dark Briar Brown 25172 2.970 C8383 13175 32835 32-17014 77 Med. Dk. Maple 72568 2.1044 C8330 13174 33284 32-16945 77 Dark Maple 72415 2.803 C8115 12271 31201 32-16777

FLAT 17 Dark Charcoal - 2.976 C8387 13257 32939 32-16878 19 Black 9433 120 4428 12812 J4-8677 32-16615 92837 22 Dark Royal Blue 15682 2.974 C8335 13253 32936 32-16875 42 Dark Grayfern 33620 2.971 C8327 13250 32935 32-16874 61 Med. Saddle Tan 25056 2.878 D8208 13145 31906 32-16856 61 Dark Saddle Tan 25058 2.880 D8217 12719 32091 32-16858 67 Dark Briar Brown 25229 2.970 C8383 13249 32934 32-16873 77 Dark Maple 72435 2.803 C8115 13258 31423 32-16803

VINYL ROOF MOLDING COLORS Sherwin- Paint Inmont Williams Martin- Number Color Name Ditzler Dupont (R.M.) Acme/Rogers Senour ------ ---------- ------- ------ ------ ----------- ------ 11 White 183 5338 12703 32503 32-26580 19 Black 120 99 4416 J4-1990 32-16082 9739 27 Med. Dark Royal Biue Met. 2.954 B8304 13159D 33175 32-26638 42 LL Grayfern Met. 2.955 B8309 13160 33186 32-26649 60 Lt. Sand Gray 2.958 B8307 13163 33178 32-26641 67 Dark Briar Brown Met. 2.960 B8305 13165 33176 32-26639 78 Dark Autumn Maple Met. 2.961 B8306 13166D 33177 32-26640 91 LL Flax F/M 2.966 C8303 13168 33181 32-26644

PAINT STRIPES

#### NOTICE: Some plants use decals or tape for strips. Sherwin- Paint Inmont Martin Williams Code Color Name Ditzler Dupont (R.M.) Senour Acme/Rogers ---- ---------- ------- ------ ------- ------ ----------- 11A White 0847 5338 2080 32-3929 L10A-2864 5644 19A Black 9300 99 A-946 3069 L10B-1738 3000/4690 27A Med. Dark Royal Blue Met. - D8304 13110 32-26624 33161 27A Med. Dark Royal Blue 15639 C8393 13282 32-26617 33154 42A Light Grayfern 32018 C8398 13283 32-26621 33158 48A Dark Grayfern Met. - B8303 13115 32-26623 33160 56A Gold Met. 24430 43516 9215 32-26314 J4-8265 25302 60A Lt. Sand Gray 3530 B8307 13120 32-26627 33164 67A Dark Briar Brown 24945 D8328 13274 32-26628 33165 67A Dark Briar Brown Met. - B8305 13127 32-26625 33162 75A Red 72128 43592 4518 32-26272 J4-7191 11892 78A Dark Autumn Maple 51127 D8329 13275 32-26629 33166 78A Dark Autumn Maple Met. - B8306 13132 32-26626 33163

ENGINE PAINT

#### NOTICE: 1983 Engine paint is available from GMWDD in the following colors in aerosol form:

Color Part Number Size ----- ------------ ---- Gas Engines Black 1051395 13 oz. Diesel Engines Diesel Blue 1052443 11 oz. 1052359 13 oz.

WHEEL COLORS

#### NOTICE: Wheels are painted with enamel therefore, please specify this type paint when ordering. Sherwin- Paint Code Williams Martin- Sem#-Gloss Color Name Dupont Inmont (R.M.) Acme/Rogers Senour ---------- ----------- ------ ------------- ----------- ------- 11 White 6338 2080 L10A-2864 30-3929 5644 15 Silver Sand Met. C8301 13100 33188 30-5256 19 Black 99 A946 L10B-1738 3069 3000/4590 22 Lt. Royal Blue Met. B8308 13106 32895 30-5229 27 Med. Dark Royal Blue Met B8304 13110 32701 30-5179 42 Lt. Grayfern Met. B8309 13114 32902 30-5234 48 Dk. Grayfern Met. B8303 13115 32702 30-5180 60 Lt.Sand Gray B8307 13120 32704 30-5182 62 Lt. Briar Brown Met. B8310 13121 32896 30-5230 67 Dark Briar Brown Met. B8305 13127 32705 30-5183 75 Spectra Red B8115 12229 31056 30-4989 78 Dark Autumn Maple Met. B8306 13132 33075 30-5245

1983 EXTERIOR PLASTIC PARTS

All 1983 Oldsmobiles have exterior parts made of various types of plastic materials that require specific procedures to obtain high quality refinishing results. Included in this bulletin is a chart listing the different exterior parts and the type of plastic materials used on 1983 models. For best results when painting is required, determine the type of plastic material from the chart; then follow the correct paint procedure, depending upon what painting material and equipment is available.

PART NAME PLASTIC TYPE SYMBOL --------- ------------ ------ FIRENZA MODELS

Front Fasica Thermoset Urethane RRIM Rear Fasica Thermoset Urethane RRIM

OMEGA MODELS

Lower Valance Panel, Front (1 pc.) Thermoplastic Urethane TPU Front End Panel, (1 pc.) Thermosetting Polyester UP Rear Bumper Fillers (5 pc.) Thermoplastic Urethane TPU Lower Valance Panel, Rear Thermoplastic Urethane TPU Front Bumper Fascia (W48 & W45) Thermoplastic Urethane RRIM Fender (Y78) Thermoset Urethans RRIM Front End Panel Thermoset Urethane RRIM Rear Wheel Flares (W45) Thermoset Urethane RRIM

CUTLASS CIERA - CUTLASS SUPREME MODELS

*Front Bumper Outer Fillers R & L Thermoplastic Elastomer TPE (2 pcs.) *Front Bumper to Fender R & L (2 pcs.) Thermoplastic Elastomer TPE Front End Panel (1 pc.) Thermosetting Polyester UP *Rear Center Fillet (1 pc.) Thermoplastic Elastomer TPE *Rear Bumper Fillers Outers (2 pcs.) Thermoplastic Elastomer TPE *Rear Body to Bumper Filler (2 pcs.) Thermoplastic Elastomer TPE Front Fasica Thermoset Urethane RRIM Rear Fasica Thermoset Urethane RRIM

*Cutlass Supreme Models Only

88 MODELS

Front Bumper to Fender R & L (2 pcs.) Thermoplastic Elastomer TPE Front Bumper Filler, Outers (2 pcs.) Thermoplastic Elastomer TPE Front End Panel (1 pc.) Thermosetting Polyester UP Rear Bumper Fillers (2 pcs.) Thermoplastic Urethane TPU Rear Center Bumper Filler (1 pc.) Thermoplastic Elastomer TPE Rear Bumper Fillers (3 pcs.) Thermoplastic Elastomer TPE (Wagon only) 98 MODELS

Front Bumper to Fender R & L (2 pcs.) Thermpplastic Elastomer TPE Front Bumper Filler, Outer (2 pcs.) Thermoplastic Elastomer TPE Front End Panel (1 pc.) Thermosetting Polvester UP Rear Bumper Fillers (2 pcs.) Thermoplastic Urethane TPU Rear Center Bumper Filler Thermoplastic Elastomer TPE

TORONADO MODELS

Front Bumpers Filler, Center (1 pc.) Thermoplastic Elastomer TPE Front Bumper Filler, Outers (2 pcs.) Thermoplastic Elastomer TPE Rear Bumper Filler, Center (1 pc.) Thermoplastic Elastomer TPE Rear Bumper Filler, Outers (2 pcs.) Thermoplastic Urethane TPU Front End Panel (1 pc.) Thermosetting Polyester UP

I. GENERAL PAINT PROCEDURE FOR EXTERIOR FLEXIBLE PLASTICS

Polyvinylchloride (PVC), Polyurethane (PUR, TPUR, RRIM, RIM) Thermoplastic Elastomer (TPE), EPDM Rubber (Supplied in Prime).

There are a multitude of finishing systems available on the market for painting and/or repairing flexible plastic parts. Following is a general outline of painting procedures including a list of available products. Refer to the manufacturer's literature available through their jobbers for details on proper mixing and application.

A. Thoroughly clean part by washing with a suitable cleaning solvent* to remove all surface contaminates.

#### NOTE: Previously painted parts that show signs of cracking, peeling or improper adhesion must be stripped before repainting. The old finish may be removed with any commercially available chlorinated solvent stripper or lacquer thinner.

#### NOTICE: Do not soak parts longer than necessary to remove the old paint to avoid swelling.

B. Scuff sand to an even dull appearance the entire surface to be painted with fine (400 grit or less) sandpaper and feather edge any damaged areas and rewash as in Step A above.

#### NOTE: Unpainted parts do not require sanding prior to painting but should be thoroughly cleaned as in Step A above.

C. Apply two (2) thin coats of primer when required per top coat manufacturer's recommendation and allow to completely dry before proceeding (for most products, approximately 30 minutes)

D. Prepare color coat according to the manufacturer's recommendation and apply sufficient double coats to develop the proper shade. For best results allow a few minutes flash time between each double coat and allow to completely dry before using.

E. Following is a list of some of the products available for painting flexible plastic.

Ditzler Elastomeric Primer - DPX844 Ditzler Flexative - DX369 (Permanent Flexible Urethane Additive) Ditzler Flex Additive - DX1798 (Non-Urethane Additive) Ditzler Delthane - DXRBO (Acrylic Enamel Hardner) Rinshed-Mason Acrylic Flex Agent 891 DuPont Dexlar Flexible Finish (Lucite tints plus Dexlar 365B Additive) Sherwin-Williams Flex Additive - V2V297 Acme/Rogers Flex Additive - 699/4699 Martin-Senour Flex Additive - 3082

*Cleaning Solvents

1. DuPont Prep-Sol 2. Rinshed-Mason Pre-Kleano 900 3. Ditzler Acryli-Clean DX330 4. Sherwin-Williams R7K156 5. Acme 88; Rogers 088 6. Martin-Senour 6383

II. NYLON - will be supplied in prime. Use the same procedure to refinish as on sheet metal parts.

III. ACRYLONNITRILE-BUTADIENE-STYRENE (ABS) - No prime required, paint with acrylic lacquer.

IV. POLYESTER PARTS (UP, PBTP) - will be supplied in prime and/or black paint. Use the same procedure to refinish or repair as on sheet metal parts.

V. POLYPROPYLENE - Interior parts.

A. Wash surface thoroughly with enamel reducer (do not use wax and grease removers)

B. Apply primer immediately and allow to dry completely before color coating.

C. Color coat with lacquer or enamel reduced and applied according to the manufacturers recommendation.

D. Materials

Cleaning Solvent - DuPont 3812S Enamel Reducer Ditzler DTE-101 or DTE-102 "Bobcat" enamel reducer Primer - DuPont 3293 GM 1052364

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.