IRREGULAR GAP @ CENTER CONSOLE AND INSTRUMENT PANEL PAD. Oldsmobile Toronado 1990

For 1990-2009 cars

# IRREGULAR GAP @ CENTER CONSOLE AND INSTRUMENT PANEL PAD

#### SUBJECT: INSTRUMENT PANEL PAD TO CENTRE CONSOLE IRREGULAR GAP (ADJUST THE I/P PAD)

#### VEHICLES AFFECTED: 1990 E

Some 1990 Oldsmobile Toronados and Trofeos may experience an irregular gap at the instrument panel pad to centre console area. Refer to Figure 1.

To correct this condition, adjust the I/P pad, utilizing the following procedures:

1. Remove knee bolster. Refer to Section 8C of the Service Information Manual.

#### NOTICE: When removing knee bolster, do not exert any downward force at upper edge on either side of steering column. Only a front-to-back horizontal force should be used to unseat top clips from instrument panel. Failure to follow these instructions may damage knee bolster beyond repair. Update page 8C-6 of Service Information Manual with this information.

2. Remove I/P steering column reinforcement plate. Refer to Section 8C of the Service Information Manual.

3. Loosen lower left and right I/P retaining screws. Refer to Figure 2.

4. Loosen retaining screws at centre I/P brace.

5. Remove defogger vent grille.

6. Loosen 3 I/P pad upper retaining screws at defogger duct area.

7. Rotate I/P pad in the necessary direction until a uniform I/P pad to centre console gap is obtained. Refer to Figure 3.

8. Tighten lower I/P retaining screws. Two persons are required; one to hold the I/P pad in proper position and one to tighten the I/P retaining screws.

9. Tighten retaining screws at centre I/P brace.

10. Tighten 3 I/P pad upper retaining screws at defogger duct area.

11. Replace defogger vent grille.

12. Replace I/P steering column reinforcement plate. Refer to Section 8C of the Service Information Manual.

13. Replace knee bolster. Refer to Section 8C of the Service Information Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.