FUEL DOOR RELEASE ESCUTCHEON LOOSE. Oldsmobile Toronado 1990

For 1990-2009 cars

# FUEL DOOR RELEASE ESCUTCHEON LOOSE

#### MODELS/YEARS 1990 TORONADO

Some 1990 Oldsmobile Toronados may experience a condition where the fuel door release escutcheon may be loose at the attachments and not aligned properly. To repair this condition use the following procedure:

Using P/N 11505850 or equivalent, a self tapping large washer head cross-recessed screw, drill through the escutcheon one inch ahead of the original screw into the body bar. (See illustration) IMPORTANT: If not using part number 11505850 use two matching black finished sheet metal screws (M 4.2 x 1.41 x 25 mm long)

#### WARRANTY INFORMATION:

Labor Operation Number: T4660 Labor Time: .2 hour Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.