WIRE WHEEL LOCKS DIFFICULT TO REMOVE. Oldsmobile Toronado 1982

For 1990-2009 cars

# WIRE WHEEL LOCKS DIFFICULT TO REMOVE

IF THE LOCK BOLT IS INSTALLED TOO TIGHTLY ON THE TORONADO MODELS, THE BOLT HEAD CAN BECOME SLIGHTLY RECESSED IN THE PLASTIC BOLT RETAINER, MAKING RE- MOVAL OF THE LOCK NUT DIFFICULT.

TO FACILITATE EASIER REMOVAL, YOU SHOULD GRIND APPROXIMATELY 1/16" OFF THE END OF THE LOCK WRENCH.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.