LOOSE QUARTER WINDOW REVEAL MOLDING/INSTALLATION PROCEDURE. Oldsmobile Toronado 1990

For 1990-2009 cars

# LOOSE QUARTER WINDOW REVEAL MOLDING/INSTALLATION PROCEDURE

Vehicls Affected: 1990 E

Some 1990 Toronados and Trofeos may have a loose quarter window reveal moulding on one or both sides of the car.

To repair this condition, first remove the loose moulding from the quarter window by pulling it off by hand. There are either eight or nine studs holding it on. Clean both the underside of the moulding and the moulding mounting surface on the quarter window with a clean, alcohol-dampened cloth and allow to air dry. Apply black urethane primer (from urethane kit P/N 9636067, or equivalent) to both surfaces and allow to dry for five minutes. apply enough urethane to fill the cavity on the back side of the moulding. Reinstall the moulding, studs and all, and tape in place. Clean excess urethane off immediately with a wax and grease removing solvent. Allow urethane to cure for four hours at room temperature before removing tape.

Use most applicable Labour Operation and time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.