AUTOMATIC DOOR LOCK OPERATION. Oldsmobile Toronado 1982

For 1990-2009 cars

# AUTOMATIC DOOR LOCK OPERATION

THE AUTOMATIC DOOR LOCKS ON 98 AND TORONADO MODELS ARE DESIGNED NOT TO OPERATE WITH THE INTERIOR LIGHTS IN THE "ON" POSITION. THE COMPLETE OPERATION CIRCUITRY AND TROUBLESHOOTING PROCEDURE CAN BE FOUND IN THE 1982 FISHER BODY MANUAL, SECTION 10 PAGE 84.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.