LTG REQUEST FOR REVIEW MAY -junE. Pontiac Acadian (Canada) 1987

For 1990-2009 cars

# LTG REQUEST FOR REVIEW MAY -junE

This bulletin addresses changes to the published Pontiac Labor Time Guide; May and June changes are attached. These changes are the result of dealer "Requests For Review" being handled by C-P-C Technical Service Activity.

These updates will be included in future 1987 Labor Time Guide revisions. In the case of past model year updates, it is recommended that this bulletin be retained with all appropriate model year Labor Time Guides, as a complete revision will not be provided.

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G H J N P T NUMBER VIN CODE

COVER, FRONT BUMPER NOTE: Applicable model years: All COLOR COAT ONE PIECE A0008 REFINISH ONE PIECE A0018 ADD: A- W/Two Tone Paint .4 AB

GRILLE NOTE: Applicable model years: All COLOR COAT A0260 .5 .3 GB GB REFINISH A0270 .6 .4 GC GC ADD: A- W/Clear Coat Paint .2 .2 CA CA

COVER, REAR BUMPER NOTE: Applicable model years: All COLOR COAT ONE PIECE A3268 REFINISH ONE PIECE A3278 ADD: A- W/Two Tone Paint .4 AB

COVER, FRONT BUMPER - REPLACE NOTE: Applicable model years: All ONE PIECE B0048 ADD: A- W/Two Tone Paint .4 AB

COVER, REAR BUMPER - REPLACE NOTE: Applicable model years: All ONE PIECE B0608 ADD: A - W/Two Tone Paint .4 AB

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G H J N P T NUMBER VIN CODE

EMBLEM, FENDER OR DOOR-REPLACE NOTE: Applicable model years: All RIGHT B7400 .2 LEFT B7401 .2

PANEL/CARRIER ASSEMBLY, C2540 3.5 INSTRUMENT CONTROL REPLACE NOTE: Applicable model years: All ADD: A- To Color Coat .5 GC

VALVE, COOLANT-REPLACE D2700 .4 NOTE: Applicable model year: 1987

WHEEL - BALANCE NOTE: Use only with 16 inch wheel option. NOTE: Applicable model year:1987 ADD: A- W/Adhesive Weights ONE .2 TWO .6 FOUR 1.3

FRONT SUSPENSION E2020 - CHECK AND/OR ALIGN NOTE: Applicable model years: All ADD: A- To Adjust Camber And/Or Caster ONE SIDE .5 BOTH SIDES .8 B- To File Struts (Each) .5

GEAR ASSEMBLY, E9720 POWER STEERING - R&R AUTO TRANS 2.6 NOTE: Applicable model years: 1986-1987

GEAR ASSEMBLY, POWER E9730 STEERING SHORT - REPLACE AUTO TRANS 2.8 NOTE: Applicable model years: 1986-1987

GEAR ASSEMBLY, POWER E9740 STEERING - REPLACE AUTO TRANS 2.6 NOTE: Applicable model years: 1986-1987

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G H J N P T NUMBER VIN CODE

GASKET,CYLINDER HEAD J0508 3.5 - REPLACE NOTE: Applicable model years:1982-87

HEAD,CYLINDER J0518 4.2 - REPLACE NOTE: Applicable model years: 1982-87

VALVE - RECONDITION J0528 4.5 OR REPLACE NOTE: Applicable model years: 1982-87

PULLEY ASSEMBLY, BELT J690 .2 IDLER - REPLACE NOTE: Applicable model year: 1986 L-4 with A/C

PISTON, ROD AND/ J1308 5.6 OR RINGS - REPLACE NOTE: Applicable model years: 1982-87

GASKET,CYLINDER HEAD J0508 3.1 - REPLACE NOTE: Applicable model years: 1984-86 w/L-4 ADD: A-With A/C .4 B- W/Cruise Control .1

VALVE - RECONDITION J0528 4.3 OR REPLACE NOTE: Applicable model years: 1984-86 w/ L-4 ADD: A-With A/C .4 B- W/Cruise Control .1

TENSIONER, SERPENTINE J0680 BELT - REPLACE NOTE: Applicable model year: 1987 L-4 .2 V-6 .7

ADAPTER AND/OR GASKET, J0960 .4 OIL FILTER - REPLACE NOTE: Applicable model years: 1987 w/ V-6

MANIFOLD, EXHAUST J0100 2.5 - REPLACE RIGHT BANK NOTE: Applicable model years:1985-87 w/V-6

MANIFOLD AND/OR GASKET, J0200 INTAKE - REPLACE 1.9 NOTE: Applicable model years: 1985-87 w/V-6

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G H J N P T NUMBER VIN CODE

GASKET, CYLINDER HEAD - REPLACE RIGHT BANK J0500 5.4 NOTE: Applicable model years: 1985-87 w/ V-6

VALVE - RECONDITION OR J0520 5.4 REPLACE NOTE: Applicable model years: 1987

SEAL, REAR MAIN BEARING J1100 1.9 - R&R AND REPACK NOTE: Applicable model years: 1984-87 w/3.8L

SEAL(S), CRANKSHAFT REAR J1120 5.9 MAIN - REPLACE NOTE: Applicable model years: 1984-86 w/L-4 and manual trans

HOUSING AND/OR GASKET, J1080 3.4 REAR MAIN SEAL- REPLACE NOTE: Applicable model years: All w/auto trans

HOSE OR PIPE, THERMOSTAT J3460 .8 BY-PASS - REPLACE NOTE: Applicable model years: 1982-86

COIL AND/OR MODULE, J4345 .7 IGNITION - REPLACE NOTE: Applicable model years: 1985-87 w/ V-6

SOLENOID, STARTER MOTOR J4580 .7 - REPLACE NOTE: Applicable model years: 1985-87 V-8 w/PFI

DRIVE ASSEMBLY, STARTER J4600 .9 MOTOR - REPLACE NOTE: Applicable model years: 1985-87 V-8 w/ PFI

MOTOR ASSEMBLY, STARTER J4620 .6 - R&R NOTE: Applicable model years: 1985-87 V-8 w/PFI

MOTOR ASSEMBLY, STARTER J4640 .6 -REPLACE NOTE: Applicable model years: 1985-87 V-8 w/ PFI

IDLE SPEED, MINIMUM J5545 - ADJUST .4 .4 .4 .4 .4 .4 .4 NOTE: Applicable model years: 1985-87

PUMP, IN TANK FUEL J5590 1.5 - R&R OR REPLACE NOTE: Applicable model years: 1987

REQUEST FOR REVIEW

VEHICLE SERIES OPERATION DESCRIPTION OPERATION A B F G H J N P T NUMBER VIN CODE

SENSOR, TRANSMISSION K2050 .3 .3 .3 .3 .3 .3 SPEED - REPLACE NOTE: Applicable model years: 1986-1987 (ALL MANUAL TRANSMISSION)

SENSOR, TRANSMISSION K6310 .3 .3 .3 .3 .3 .3 .3 .3 .3 SPEED - REPLACE NOTE: Applicable model years: 1986-1987 (ALL AUTOMATIC TRANSMISSION)

GAGE AND/OR 'O' RING, L1200 1.0 FUEL (TANK UNIT) - REPLACE NOTE: Applicable model years: 1985-87 POLICY: T

SHIELD, EXHAUST MANIFOLD L2380 1.7 PIPE HEAT - REPLACE NOTE: Applicable model years: 1985-87 w/ V-6

SWITCH, ENGINE OIL N2220 .9 PRESSURE - REPLACE NOTE: Applicable model years: 1985-87 w/ V-6

MODULE - REPLACE N4829 HEADLAMP CLOSURE PANEL RIGHT .6 LEFT .6 NOTE: Applicable model years: 1985-87

PIPE, POWER STEERING HYDRALIC - REPLACE PRESSURE E8900 EXC 6-CYL .7 NOTE: Applicable model year: 1987

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.