Assembly, Door - Inner Front. Pontiac Demonstrator 1985

For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Notice .
1 | Bezel Assembly, Front Side Door Window Multifunctional Switch Assembly TIP: Use a small flat-bladed tool to release the bezel retainer.
2 | Handle, Inside Front Side Door TIP: Use a small flat-bladed tool to release the bezel retainer.
3 | Panel, Trim Front Door Tip: Push the center of the trim panel fasteners to remove.
4 | Extension, Front Door Trim Panel Upper Tip: Pull straight up and out from the door trim panel.
5 | Deflector, Front Side Door Water
6 | Bolt, Front Side Door Window Regulator (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten: to 10 N·m (89 lb ft)
7 | Regulator Assembly, Front Side Door Window Tip: Loosen the window regulator bolts, lift up and out from the key slots.
8 | Speaker, Front Side Door Radio Tip: Drill out the rivets.
9 | Handle, Front Side Door
10 | Harness, Front Side Door Wiring
11 | Rod, Front Side Door Locking
12 | Screw, Front Side Door Lock (Qty: 3) Tighten: to 10 N·m (89 lb ft)
13 | Lock, Front Side Door
14 | Weatherstrip, Front Side Door
15 | Seal, Front Side Door Window Inner
16 | Seal, Front Side Door Window Outer
17 | Weatherstrip, Front Side Door Window
18 | Window, Front Side Door
19 | Door, Front Side Window Replacement, refer to Front Side Door Window Replacement for additional information.