Scan Tool Output Controls. Pontiac Demonstrator 1985

For 1990-2009 cars

Scan Tool Output Control | Additional Menu Selection | Description
--- | --- | ---
Access Relay Output Status | Accessory Relay Control | The BCM activates the accessory relay when you select ON. The accessory relay should remain On for 30 seconds.
Driver Door Unlock | Door Lock Test | The BCM pulses the driver door lock actuator when you select ON. The driver door should unlock.
Passenger Door Unlock | Door Lock Test | The BCM pulses the passenger door lock actuators when you select ON. All of the doors, except the driver door, should unlock.
Lock All Doors | Door Lock Test | The BCM pulses all of the door lock actuators when you select ON. All of the doors should lock.
Rear Defog Relay Command | Defogger Control | The BCM activates the rear defog relay when you select ON. The rear defog relay should remain On for 60 seconds.