Power Window Lockout Function Inoperative. Pontiac Demonstrator 1985

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Power Window Schematics Connector End View Reference: Power Door Systems Connector End Views
1 | Did you perform the Vehicle Diagnostic System Check? | Go to Step 2 | Go to in Vehicle DTC Information
2 | Verify that the power windows lockout function is inoperative. Does the power windows lockout function operate normally? | Go to in Wiring Systems | Go to Step 3

3

1. Disconnect the driver window switch.
2. Turn ON the ignition, with the engine OFF.
3. Probe the power window master switch lockout signal circuit of the driver window switch with a test lamp that is connected to a good ground.

Does the test lamp illuminate?

Go to Step 4

Go to Step 5

4 | Repair the short to voltage in the power window master switch lockout signal circuit. Refer to in Wiring Systems. Did you find and correct the condition? | Go to Step 7 | Go to Step 5
5 | Inspect for a poor connections at the harness connector of the driver window switch. Refer to and in Wiring Systems. Did you find and correct the condition? | Go to Step 7 | Go to Step 6
6 | Replace the driver window switch. Refer to Front Side Door Window Switch Replacement - Left Side . Did you complete the replacement? | Go to Step 7 | --
7 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2