OIL PUMP ROTOR AND SLIDE UPDATED P/N'S LISTED 125/125C. Pontiac J2000 1982

For 1990-2009 cars

# OIL PUMP ROTOR AND SLIDE UPDATED P/N'S LISTED 125/125C

THIS BULLETIN SUPERCEDES BULLETIN HM 83-10, WHICH SHOULD BE DESTROYED. WHEN SERVICING THE OIL PUMP ROTOR AND SLIDE ON A THM 125/125C TRANSAXLE, REFER TO THE APPROPRIATE SERVICE MANUAL, WHICH DESCRIBES THE FOLLOWING PROCEDURE: USE A MICROMETER TO MEASURE THE ORIGINAL PUMP ROTOR AND/OR SLIDE THICKNESS. REFER TO FIGURE 1. TAKE MEASUREMENT ON A FLAT, UNDAMAGED SURFACE. USE THE ORIGINAL PART MEASUREMENT TO SELECT THE PROPER SERVICE PACKAGE FROM THE FOLLOWING CHARTS: 1980-1981 THM 125 (ORDER ROTOR AND SLIDE SEPARATELY) ROTOR (MM) PART NUMBER SLIDE (MM) PART NUMBER 17.943-17.955 8653961 17.955-17.967 8631800 17.956-17.968 8653962 17.968-17.980 8631801 17.969-17.981 8653963 17.981-17.993 8631802 17.982-17.994 8653964 17.994-18.006 8631803 17.995-18.008 8653965 18.007-18.020 8631804 1982-1986 THM 125C (ORDER ROTOR AND SLIDE AS COMPLETE PACKAGE) ROTOR (MM) SERVICE PACKAGE NUMBER 17.943-17.956 8652903 17.956-17.969 8652904 17.969-17.982 8652905 17.917-17.930 8652906 17.930-17.943 8652907

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.