CENTER HUB ORNAMENT REMOVAL AND INSTALLATION. Pontiac J2000 1982

For 1990-2009 cars

# CENTER HUB ORNAMENT REMOVAL AND INSTALLATION

THE CENTER ORNAMENT ON CUTLASS CIERA AND FIRENZE MODELS EQUIPPED WITH PO3 RALLYE WHEELS SHOULD NOT BE REMOVED WITH THE WHEEL LUG NUTS IN PLACE. TO REMOVE THE CENTER ORNAMENT, THE LUG NUTS MUST BE REMOVED FIRST. TO INSTALL THE CENTER ORNAMENT, INSTALL AND TIGHTEN THE LUG NUTS. THEN INSTALL THE CENTER ORNAMENT WITH A RUBBER MALLET.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.