PARKING BRAKE ADJUSTMENT PROCEDURE INFORMATION. Pontiac J2000 1982

For 1990-2009 cars

# PARKING BRAKE ADJUSTMENT PROCEDURE INFORMATION

CIMARRON PARKING BRAKE ADJUSTMENT PROCEDURE: THE FOLLOWING PROCEDURE (WHICH IS NOT INCLUDED IN THE 1982 SERVICE MANUAL) SHOULD BE FOLLOWED WHEN ADJUSTING THE PARKING BRAKE ON 1982 CIMARRONS: 1.APPLY PARKING BRAKE LEVER EXACTLY 5 CLICKS. 2.RAISE AND SUITABLY SUPPORT CAR. 3.CHECK THE EQUALIZER NUT GROOVE TO SEE THAT IT IS LIBERALLY LUBRICATED. IF NOT LUBRICATED, USE CHASSIS GREASE GM PART NUMBER 1052497 OR EQUIVALENT. 4.TIGHTEN ADJUSTING NUT UNTIL RIGHT REAR WHEEL CAN JUST BE TURNED REARWARD USING TWO HANDS BUT IS LOCKED WHEN FORWARD ROTATION IS ATTEMPTED. 5.WITH THE PARKING BRAKE DISENGAGED, THE REAR WHEELS MUST TURN FREELY IN EITHER DIRECTION WITH NO BRAKE DRAG. 6.REMOVE SUPPORT AND LOWER CAR.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.