INSTRUMENT PANEL SPACER BRACKET REPLACEMENT. Pontiac J2000 1982

For 1990-2009 cars

# INSTRUMENT PANEL SPACER BRACKET REPLACEMENT

#### SUBJECT MODEL LEFT HAND INSTRUMENT SOUND INSULATOR ASSEMBLIES ARE BEING REPLACED BY A SPACER BRACKET, PART NO. 14091377, TO FACILITATE THE USE OF THE 1983 SOUND INSULATORS ON THE 1982 INSTRUMENT PANEL PAD. THIS BRACKET MUST BE USED AT LEFT HAND REAR ATTACHMENT OF THE SOUND INSULATOR ASSEMBLY. FIGURE SHOWS THE NEW BRACKET AS INSTALLED WITH A 1982 INSTRUMENT PANEL AND THE 1983 DESIGN SOUND INSULATOR ASSEMBLY.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.