UPPER RADIATOR HOSE CLEARANCE MAY CONTACT SPARK PLUG SHIELD. Pontiac J2000 1982

For 1990-2009 cars

# UPPER RADIATOR HOSE CLEARANCE MAY CONTACT SPARK PLUG SHIELD

UPPER RADIATOR HOSE CLEARANCE- 1982 J2000 EQUIPPED WITH 1.8L OHC-FI ENGINE (CODE O) WHEN PERFORMING REGULAR MAINTENANCE OR REPAIR SERVICES IN THE AREA OF THE UPPER RADIATOR HOSE IT IS IMPORTANT THAT CLEARANCE BE MAINTAINED BETWEEN THE HOSE AND THE NUMBER ONE SPARK PLUG WIRE SHIELD. IF THE HOSE IS INSTALLED INCORRECTLY OR THE SHIELD BENT, A CONTACT CAN BE MADE BETWEEN THEM. THIS CONTACT, DUE TO THE ENGINE FORE AND AFT ROLL, COULD RESULT IN A CUT HOSE AND LOSS OF COOLANT: AFTER SERVICE OPERATIONS IN THIS AREA, INSPECT FOR CLEARANCE BETWEEN THE TWO PARTS. CLEARANCE SHOULD BE MAINTAINED AT 12.7MM(5") TO ASSURE CONTACT IS NOT MADE. THE UPPER EDGE OF THE SPARK PLUG SHIELD CAN BE TURNED DOWNWARD IF NECESSARY TO GAIN ADDITIONAL CLEARANCE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.