DRIVE BELT LIFE INCREASE PULLEY TORQUE COMPENSATOR. Pontiac Parisienne (Canada) 1983

For 1990-2009 cars

# DRIVE BELT LIFE INCREASE PULLEY TORQUE COMPENSATOR

A CRANKSHAFT PULLEY TORQUE COMPENSATOR, SIMILAR TO THAT USED ON THE V6 DIESEL ENGINE, IS NOW BEING USED IN PRODUCTION ON THE 5.7L V8 DIESEL ENGINE. THE TORQUE COMPENSATOR REDUCES THE TORQUE VARIATIONS BEING TRANSMITTED TO THE DRIVE BELT AND WILL INCREASE DRIVE BELT LIFE. THE TORQUE COMPENSATOR IS AVAILABLE FOR 1980 THROUGH 1983 5.7L V8 DIESEL MODELS, WITH A/C, THAT USE A TWO (2) GROOVE CRANKSHAFT PULLEY. THE TORQUE COMPENSATOR, AND FOUR (4) BOLTS REQUIRED FOR INSTALLATION ARE AVAILABLE THROUGH WDDGM. P/N 22521773.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.