DIESEL BLACK SMOKE 1981-82 VEHICLES. Pontiac Parisienne (Canada) 1981

For 1990-2009 cars

# DIESEL BLACK SMOKE 1981-82 VEHICLES

WHEN INVESTIGATING COMMENTS OF EXCESSIVE BLACK SMOKE FROM DIESEL ENGINES AT 1/3 TO 1/2 THROTTLE OPENINGS, CHECK OPERATION OF E.P.R. AND V.R.V VALVES. EXCESSIVE E.P.R. PRESSURE CAUSES HIGH E.G.R. FLOW, DILUTING INTAKE AIR WITH EXHAUST GAS AND STARVING ENGINE FOR OXYGEN RESULTING IN BLACK SMOKE. ANOTHER SOURCE OF INTAKE AIR DILUTION COULD BE A LEAK AT EITHER OR BOTH SIDES OF THE INTAKE CROSSOVER GASKET.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.