BINDING/DISCONNECTED MAN.SHAFT NEW ROD END CLIP THM700-R4. Pontiac Parisienne (Canada) 1983

For 1990-2009 cars

# BINDING/DISCONNECTED MAN.SHAFT NEW ROD END CLIP THM700-R4

BEGINNING WITH SERIAL NUMBER 3TC152D ALL THM 700-R4 TRANSMISSIONS ARE BEING BUILT WITH A NEW ROD END CLIP (PART NUMBER 8654037) (SEE FIG.1). NOTICE: WHEN INSTALLING THE OUTSIDE MANUAL LINKAGE NUT ON A THM 700-R4 TRANSMISSION DO NOT USE AN AIR POWERED TOOL. USING AN AIR POWERED TOOL TO PERFORM THIS FUNCTION MAY ROTATE THE MANUAL SHAFT WITH ENOUGH FORCE TO MISLOCATE THE ROD END CLIP. IF THIS CLIP BECOMES LOOSE OR MISLOCATED, IT WILL BE NECESSARY TO REMOVE THE OIL PAN TO EITHER REPLACE OR REINSTALL THE ROD END CLIP. SEE ILLUSTRATION

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.