2-4 SERVO PIN TORQUE SPEC SERVICE MANUAL CORRECTION. Pontiac Parisienne (Canada) 1983

For 1990-2009 cars

# 2-4 SERVO PIN TORQUE SPEC SERVICE MANUAL CORRECTION

The 2-4 Servo Pin Selection Procedure found on page 700-R4-8 of the Transmission Disassembly Section, reflects the incorrect torque specification in Step C. It should state, "install a torque wrench and apply 11 N.m (100 in. lbs.)".

The following 1983 Shop Manuals are affected:

1983 General Carline Information 1983 Parisienne

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.