THM 2004R TURBINE SHAFT SOLID SEAL RING REPLACEMENT. Pontiac Parisienne (Canada) 1981

For 1990-2009 cars

# THM 2004R TURBINE SHAFT SOLID SEAL RING REPLACEMENT

PLEASE AMEND THE 7A6-SECTION OF THE 1981 NEW MODEL PRODUCT INFORMATION AND SERVICE MANUALS TO INCLUDE THE FOLLOWING SOLID TEFLON TURBINE SHAFT SEAL REPLACEMENT PROCEDURE (FIGURE 1): 1.IF THE SOLID TEFLON SEAL RING REQUIRES REPLACEMENT, REMOVE IT BY CAREFULLY CUTTING IT WITH A KNIFE. 2.PLACE THE SEAL INSTALLER (J-29696-1) OVER THE TURBINE SHAFT AND LUBRICATE THE INSTALLER WITH PETROLATUM (FIGURE 2). 3.PLACE THE SOLID OIL SEAL RING OVER THE SEAL INSTALLER AND CAREFULLY, BUT QUICKLY SLIDE THE SEAL DOWN TO THE SEAL RING GROOVE. REMOVE THE SEAL INSTALLER (FIGURE 3). 4.LUBRICATE THE INSIDE OF THE SIZING TOOL (J-29696-2) WITH PETROLATUM. PUSH THE SIZING TOOL DOWN OVER THE SEAL AND TURN. REMOVE THE SIZING TOOL AND INSPECT THE SEAL TO BE SURE THAT IT IS PROPERLY SEATED IN THE GROOVE (FIGURE 3).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.