FLYWHEEL-CONVERTER BOLTS REVISED TORQ SPECIFICATIONS. Pontiac Parisienne (Canada) 1981

For 1990-2009 cars

# FLYWHEEL-CONVERTER BOLTS REVISED TORQ SPECIFICATIONS

FLYWHEEL TO TORQUE CONVERTER BOLT TORQUE HAS BEEN CHANGED FROM 40-54 NM 35-40 LB/FT TO 55-70 NM 41-52 LB/FT. ALSO RETORQUE THE FIRST BOLT AFTER ALL THREE (3) HAVE BEEN TORQUED.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.