ENG.CODE 24,34,32 SHOP MANUAL DIAGNOSTICS CORRECTION. Pontiac Phoenix 1982

For 1990-2009 cars

# ENG.CODE 24,34,32 SHOP MANUAL DIAGNOSTICS CORRECTION

THE FOLLOWING CORRECTION SHOULD BE MADE TO SUBJECT CHART SHOWN ON PAGE 6E2-20, FIGURE 6E2-25, SECTION 6E2 OF THE 1982 CITATION-CELEBRITY SHOP MANUAL (ST365-82) AND ON PAGE 6E-21, FIGURE 6E-27, SECTION 6E OF THE 1982 CORVETTE SHOP MANUAL (ST364-82). WHEN CHECKING PIN 20, CKT 419 BACK PROBE CONNECTOR WITH TEST LIGHT TO 12 VOLTS NOT TO GROUND. PIN 20 IS GROUND AND TEST LIGHT WOULD NOT COME "ON" UNDER ANY CONDITION.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.