REVISED FUEL FILTER REPLACE PROCEDURES 1981 X. Pontiac Phoenix 1981

For 1990-2009 cars

# REVISED FUEL FILTER REPLACE PROCEDURES 1981 X

THE FOLLOWING REVISED PROCEDURE WILL AID TECHNICIANS IN THE REPLACEMENT OF THE FUEL FILTER ELEMENT ON 1981 OMEGA SERIES WITH L-4 ENGINES. 1.REMOVE AIR CLEANER ASSEMBLY. 2.DISCONNECT LARGE CARBON CANISTER BOWL VENT HOSE FROM THE CARBURETOR. 3.REMOVE SCREW RETAINING 3-HOSE MOLDED VACUUM HARNESS FROM 3 CANISTER PIPES, AND MOVE THE PIPES UP AND OUT OF THE WAY. 4.LOOSEN THE A.I.R. PUMP ADJUSTING BOLT AND MOVE THE PUMP ASSEMBLY FORWARD FOR CLEARANCE. 5.DISCONNECT THE CHOKE COIL ELECTRICAL CONNECTOR AND FUEL INLET LINE CONNECTION. REMOVE THE FUEL FILTER NUT, FILTER, AND SPRING. USE A LINE WRENCH TO BREAK LOOSE AND TIGHTEN THE FUEL INLET LINE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.