COLD IDLE ROUGHNESS NEW PROM INFORMATION. Pontiac Phoenix 1983

For 1990-2009 cars

# COLD IDLE ROUGHNESS NEW PROM INFORMATION

Some 1983 1/2 Phoenix with 2.5L engine, automatic transaxle, and one-board ECM (previously covered in Bulletin 83-1-102, Section 6), may experience a rough idle when the engine is cold.

This condition may be corrected by installing a new PROM, Part Number 1226725.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.