SUN VISOR LOOSE/WILL NOT HOLD POSITION (INSTALL SLEEVE). Pontiac Safari Wagon 1988

For 1990-2009 cars

# SUN VISOR LOOSE/WILL NOT HOLD POSITION (INSTALL SLEEVE)

SUN VISOR LOOSE AND WILL NOT HOLD POSITION

#### VEHICLES AFFECTED: 1986-1988 'B' SERIES ------------------

Owner comments on B-car sun visors that are loose and will not hold position can be addressed by replacing the sleeve, P/N 8740843 with a new thicker sleeve, P/N 17927383.

1. Loosen tensioning screw and remove sunshade from support.

2. Extract clear plastic sleeve from sunshade using needle nose pliers and replace with new sleeve (black plastic), P/N 17927383.

3. Check rod on support assembly to be sure it does not turn within the support. If rod turns replace support assembly.

4. Reinstall sunshade and check for proper operation.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim 0.3 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.