Defroster Grille Popping Noise Encountered During Cold Temperatures (Lubricate Both Retaining Clips and Clip Attachment Points). Saturn L Series 2002

For 1990-2009 cars

# Defroster Grille Popping Noise Encountered During Cold Temperatures (Lubricate Both Retaining Clips and Clip Attachment Points)

Subject: | Defroster Grille Popping Noise Encountered During Cold Temperatures (Lubricate Both Retaining Clips and Clip Attachment Points)

Models: | 2000-2003 Saturn L-Series Vehicles

Attention: | Technician

### Condition

Customers may comment on a popping noise coming from the defroster grille while vehicle is warming up in cold temperatures.

### Cause

Thermal expansion of the plastic may cause the defroster grille to exhibit popping noise conditions.

### Correction

Lubricate both retaining clips found in the dash panel and the clip attachment points located on the defroster grille with an even coat of Dupont® Krytox® Performance Lubricant GPL 105, or equivalent. This can be purchased from Dupont, Miller-Stephenson or similar lubricant distributors. (Saturn retailers located in Canada should order P/N 03634770 (29 ml) that is available from GMSPO.)

### Procedure:

Windshield Defroster Grille

Removal:

1. Pull up defroster grille to disengage retaining clips.
2. Remove defroster grille.
3. Lubricate both retaining clips found in the dash panel and the clip attachment points located on the defroster grille with an even coat of Krytox®.

Installation:

Snap defroster grille into place.

### Claim Information:

To receive credit for this repair during the warranty coverage period, submit a claim through the Saturn Dealer System for C2368 (Outlet, Grille Defroster, Center-Replace), or if another procedure is performed, refer to the appropriate Electronic Labor Time Guide for the correct Labor Operation Code and Time.