HEADLINER SAGS AT REAR ADD HOOK & LOOP HEADLINER. Saturn Saturn 1991

For 1990-2009 cars

# HEADLINER SAGS AT REAR ADD HOOK & LOOP HEADLINER

#### SUBJECT: Headliner Sags at Rear (Add Hook and Loop Material to Headliner)

Due to the addition of "MODELS AFFECTED" with a VIN breakpoint, this bulletin supersedes bulletin 91 - T - 13, which should be discarded.

#### MODELS AFFECTED: 1991 and 1992 vehicles built before vehicle identification number (VIN) NZ102000.

CONDITION: Customer may experience a condition of headliner sagging at rear window.

CORRECTION: To correct the gap between headliner and rear window, perform the following procedure:

#### PROCEDURE:

--------- NOTICE: When doing repairs, be careful not to bend the headlining trim finish panel. If headlining trim finish panel becomes bent, it may break and leave a wrinkle.

1. Carefully pull down on rear of headlining trim finish panel, disengaging two hook and loop attaching strips.

2. Mark location on backside of the headlining trim finish panel, 114 mm (4.5 in.) forward of the center rear edge.

3. Clean area adjacent to mark on rear roof bow using 3M General Purpose Cleaner #8964 (or equivalent).

4. Apply 3M Plastic and Emblem Adhesive #8061 (or equivalent), to area shown. Allow to dry for about 10 minutes.

#### IMPORTANT: Use a sufficient amount of adhesive to penetrate into the first underlying layer of the headlining trim finish panel.

5. Using 3M Hook and Pile #6480 (or equivalent hook and loop material), attach a 51 mm (2 in.) long strip to adhesive location. Make sure protective tape is removed from both sides of the hook and loop material before installing.

6. Install headlining trim finish panel using sufficient pressure on all hook and loop locations to make sure of proper engagement of the hook and loop material.

CLAIM INFORMATION: To receive credit for this repair, submit a claim through the Saturn Dealer System.

Labor Case Operation Type Description Code Time ------------------------------------------------------ VW Add hook and loop material to T9512 0.3 hrs roof and headliner

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.