SERVICE MANUAL UPDATE - BODY / COLLISION REPAIR. Saturn Saturn 1991

For 1990-2009 cars

# SERVICE MANUAL UPDATE - BODY / COLLISION REPAIR

#### SUBJECT: 1991-1992 Body/Collision Repair, and Specifications Service Manual Updates (Headlamp Cover Panel Assembly Gap Specification).

#### MODELS AFFECTED: All 1991 and 1992 Saturn SC Coupes

PURPOSE: The "1991-1992 Body/Collision Repair" and "1991-1992 Revised Specifications Service Manual" were published without the gap specifications for the headlamp cover panel assembly for the Saturn SC Coupe. Please add the following gap specifications to page BDGI 40 in the "General Information" section of the "1991-1992 Body/Collision Repair Service Manual" and to page RFSP 64 of the "1991-1992 Revised Specifications Service Manual."

Location Clearance Gap mm (in.) Flushness mm (in.) -------- ---------------------- ------------------ Headlamp cover panel 6.0 + 1.0 parallel within 1.0 +0.0/-1.0 (+O.O/-O.04) assembly to hood (0.24+O.04 parallel within 0.24)

Headlamp cover panel 5.0+1.0 parallel within 1.0 +0.75/-1.75 (+O.03/-O.07) assembly to fender (0.20+O.04 parallel within 0.24)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.