1992 MODEL PAINT INFORMATION LIST OF COLORS/SUPPLIERS/CODES. Saturn Saturn 1992

For 1990-2009 cars

# 1992 MODEL PAINT INFORMATION LIST OF COLORS/SUPPLIERS/CODES

#### SUBJECT: 1992 MODEL PAINT INFORMATION

The listings of 1992 paint codes contained in this bulletin will enable retailers to order the necessary paint materials required for proper field repairs.

The list of colors indicates the suppliers' ordering codes for exterior and interior colors.

At this time, all Saturn vehicles are built at the Spring Hill, Tennessee manufacturing facility and painted with a base coat/clearcoat paint system.

Paint manufacturers such as PPG, DuPont, R-M/Glasurit, Sherwin Williams-Martin Senour-Acme produce service paint which could perform satisfactorily for field repairs. Paint suppliers in your area can provide you with information regarding these materials.

The paint listed in this bulletin is available from local paint suppliers.

The Service Parts Identification (SPID) label illustrated in Figure on page 3 is located on the inside of the deck lid. This label contains the paint codes needed to identify the paint materials for field repairs. This label identifies the paint code along with the WA# for that paint code. It is equally important to use this WA# along with the paint code to identify the correct repair materials. Care should be taken to transfer the SPID label or its information if the panel to which the label is affixed requires replacement. Replacement SPID labels are not available.

All 1991 Saturn vehicles employ composite body panels on the vertical surfaces of the automobile. Included in this bulletin is a chart identifying each type of material and where it is used.

Plastic Type Symbol Application ------------- ------ -------------------- GTX 910 PPE+PA Fenders and Quarters PULSE ABS+PC Doors and Rockers Thermoplastic Olefin TPO Front and Rear Fascias

A. Rigid Plastic Refinishing-GTX and PULSE

1. Same procedures as used for sheetmetal.

2. Flex additives are not required when using urethane paint systems.

3. Avoid lacquer finishes and aggressive solvents and pre-cleaners.

B. Flexible Plastic Refinishing-TPO

1. A Polyoflin adhesion promoter such as 3M 05907 or equivalent is required over all unpainted surfaces.

2. Flexible additives, used per manufacturer's recommendations, are required in primer surfacer and clearcoat.

C. Structure Painting and Touch-Up

1. Structural components are painted black with 50% gloss. PPG DP90 or equivalent is recommended.

2. Door openings and upper door frames are finished with a black 50% gloss top coat finish.

#### 1992 MODEL PAINT INFORMATION EXTERIOR

Sherwin- Williams Paint Color ACME-Rogers Code Name WA# R-M PPG Dupont Martin-Senour Glasurit ---- --------------- ---- ----- ---- ----- -------- -------- 13 Bright Silver Poly 9566 21056 4330 B9149 44118 GM-9566 15 Medium Gray Poly 9561 21064 4331 B9150 44119 GM-9561 20 Saturn Blue Poly 9557 21060 4332 B9151 44121 GM-9557 24 Bright Blue Poly 9564 21065 4333 B9152 44122 GM-9564 25 Aquamarine Poly 9998 22268 4532 B9259 45993 GM-9998 28 Black Sapphire Poly 9559 21062 4334 B9153 44123 GM-9559 39 Drk. Green Poly 9560 21063 4335 B9154 44125 GM-9560 40 White 9563 21055 4336 B9155 44126 GM-9563

41 Black 8555 13572 4337 99 33756 54-1240 90-5760 M-S 51 Drk. Antelope Poly 9555 21061 4339 B9157 44128 GM-9555 75 Brilliant Red Poly 9554 21058 4340 B9158 44134 GM-9554 Bright Red 9652 21057 4341 B9159 44135 GM-9652

#### 1992 MODEL PAINT INFORMATION INTERIOR

Sherwin- Paint Glasurit Martin- Williams Code Name WA# R-M PPG Dupont Senour ACME-Rogers ---- ------- ---- -------- ------- ------ ------- -------- 12DN Graphite 7701 13199S/G DIU-33870 C8345 16963FLT 33767FLT 16042FLT UCV-2-1020 16905S/G 32989S/G

16DN Neutral 5302 22236 UCV-2-1484 C9267 46488S/G 46488S/G Gray DIU-35395

2ODN Very Dk. 8841 17094S/G DIU-16202 C8770 36571FLT 36571FLT Sapphire 17095FLT UCV-2-1215 36479S/G 36479S/G

65BN Medium 9102 18049S/G DIU-26252 C8806 38602FLT 38602FLT Antelope 18048FLT UCV-2-1290 38219S/G 38219S/G

65CN Dk. 9245 18053S/G DIU-26255 C8809 38222FLT 38222FLT Antelope 18052FLT UCV-2-1294 38384S/G 38384S/G

FLT = Flat (No Gloss) S/G = Semi-Gloss

For Glasurit numbers use the R-M five digit number with the prefix "GM" and no suffix.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.