New Transaxle Magnets. Saturn Saturn 1995

For 1990-2009 cars

# New Transaxle Magnets

Subject: | Service Information on New Automatic Transaxle Magnets

Models: | 1995 Saturns equipped with MP6/MP7 automatic transaxles built after VIN SZ190218

### Purpose

A new Automatic transaxle magnet has been added to two locations on all automatic transaxles built after the above mentioned VIN. The new automatic transaxle magnet has been added to the pressure filter and the suction filter. The addition of these two automatic transaxle magnets increases capability for removing metal particles from the automatic transaxle hydraulic fluid.

When servicing an automatic transaxle pressure filter, remove the automatic transaxle magnet from the pressure filter, wipe it clean and reinstall. When performing repairs on the automatic transaxle and the case is disassembled, remove the automatic transaxle magnet from the bottom side of the suction filler, wipe it clean, and position it back in its original location. It is not necessary to replace the magnet(s) each time the automatic transaxle is serviced.

Important: The new automatic transaxle magnet will be available for service late in the 1995 model year.