DIESEL PUMP GEAR CLEARANCE SPEC. CHANGE. Buick Electra Estate Wagon 1981

For 1990-2009 cars

# DIESEL PUMP GEAR CLEARANCE SPEC. CHANGE

THE 1981 SERVICE MANUAL DIESEL SECTION 6A5-69, INJECTION PUMP GEAR END PLAY CLEARANCE IS .002 TO .006. MAKE NOTE OF THIS CHANGE IN YOUR SERVICE MANUAL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.