INT./EXT. PAINT CODES- MOLDINGS AND STRIPING COLORS. Buick Electra Estate Wagon 1983

For 1990-2009 cars

# INT./EXT. PAINT CODES- MOLDINGS AND STRIPING COLORS

#### MODELS AFFECTED: 1983 Century

The purpose of this bulletin is to provide an aid for determining the required 1983 Fisher Body matching color standards for lacquer, waterborne enamel, and high solids enamel.

On 1983 Centurys assembled in Oklahoma City, match the lacquer standards for color, even though the body plate will show a "W" after the paint code (i.e. 15W) indicating the paint technology as being waterborne enamel. See chart for Oklahoma City lacquer color standards.

Chart #1 Oklahoma City Lacquer Color Standards

Sherwin Williams Martin Rinshed Color GM Code DuPont Acme/Rogers Senour Mason Ditzler

Silver Sand Gray Met. 15 C8301 33188 30-5256 13100 3520

Lt. Royal Blue Met. 22 B8308 32895 30-5229 13106 3522

Med. Dk. Royal Blue Met. 27 B8304 32701 30-5179 13110 3525

Lt. Grayfern Met. 42 B8309 32902 30-5234 13114 3526

Dk. Grayfern Met. 48 B8303 32702 30-5180 13115 3528

Lt. Briar Brown Met. 62 B8310 32896 30-5230 13121 3531

Dk. Briar Brown Met. 67 B8305 32705 30-5183 13127 3534

Lt. Maple Met. 73 B8108 31055 30-4988 13522 3331

Dk. Autumn Maple Met. 78 C8310 33075 30-5245 13132F 3553

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.