C-68 AIR CONDITIONING SYSTEM WON'T MAINTAIN CONSTANT TEMP. Buick Electra/Park Avenue 1982

For 1990-2009 cars

# C-68 AIR CONDITIONING SYSTEM WON'T MAINTAIN CONSTANT TEMP

CONDITION: SYSTEM OVER REACTS TO TEMPERATURE SETTINGS. IT IS MOST NOTICEABLE WHEN SET AT A VERY LOW TEMPERATURE OR VERY HIGH TEMPERATURE . THE PASSENGER COMPARTMENT GETS EITHER TOO COLD, OR TOO HOT FOR TEMPERATURE SETTING. CAUSE: MISSING IN-CAR SENSOR COVER (SEE ILLUSTRATION). CORRECTION: INSPECT VEHICLE FOR IN-CAR SENSOR COVER. IF THE COVER IS MISSING, ORDER PART NUMBER 1259773 (COVER) AND INSTALL. PROCEDURE: 1.REMOVE RIGHT SIDE INSTRUMENT PANEL TRIM PLATE BY PULLING STRAIGHT OUT. 2.REMOVE FOUR (4) SCREWS FROM DEFROSTER GRILL (TWO ON EACH SIDE). 3.REMOVE TWO (2) SCREWS FROM PADDED INSTRUMENT COVER SIDES, (ONE ON EACH SIDE). 4.REMOVE FIVE (5) 7MM SCREWS FROM UNDER FRONT OF PADDED INSTRUMENT PANEL COVER. 5.LIFT PADDED INSTRUMENT PANEL COVER AND CHECK FOR IN-CAR SENSOR COVER, INSTALL AS NECESSARY. 6.TO ASSEMBLE, REVERSE PROCEDURE. WARRANTY INFORMATION: LABOR OPERATION T5048 LABOR TIME .4 HRS. TROUBLE CODE 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.