FRONT DOOR WINDOW FRAME RATTLE NEW WINDOW FRAME- REAR BUMPER. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# FRONT DOOR WINDOW FRAME RATTLE NEW WINDOW FRAME- REAR BUMPER

A CONDITION DESCRIBING A RATTLE ON ROUGH ROADS FROM THE CENTER PILLAR UPPER AREA OR UPPER REAR OF FRONT DOOR FRAME AREA MAY BE EXPERIENCED. A NEW WINDOW FRAME UPPER REAR RUBBER (OVERSLAM) BUMPER WAS IMPLEMENTED IN PRODUCTION IN JULY, 1984. THE ABOVE CONDITION MAY BE DIAGNOSED BY, PUSHING OUT ON REAR OF DOOR UPPER WINDOW FRAME , AND IF THE NOISE STOPS, REPLACE BUMPER WITH P/N 20325056 IN GROUP 14.651 FROM GMWDD.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.