A/C- INSUFFICIENT COOLING MISSING HEAT SHIELD. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# A/C- INSUFFICIENT COOLING MISSING HEAT SHIELD

SOME EARLY PRODUCTION 1985 "C" MODELS MAY HAVE BEEN BUILT WITHOUT THE SUBJECT HEAT SHIELD. IF AN AIR CONDITIONING FAILURE IS TRACED TO THE IDLE SPEED POWER STEERING PRESSURE SWITCH; CHECK FOR PRESENCE OF HEAT SHIELD (FIGURE 1). INSTALL HEAT SHIELD P/N 25522467 AND REPLACE SWITCH. THE SHIELD AFFORDS ADDED PROTECTIONS IN HOT AMBIENTS FROM EXHAUST HEAT AND SWITCH FAILURES.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.