REVISE FUEL PUMP CONNECTOR- LOCATION SERVICE MANUAL UPDATE. Buick Electra/Park Avenue 1986

For 1990-2009 cars

# REVISE FUEL PUMP CONNECTOR- LOCATION SERVICE MANUAL UPDATE

1986 SERVICE MANUAL CORRECTION

#### MODELS AFFECTED: 1986 "C", "H" SERIES ---------------

#### NOTE: This information supersedes all previously published Service Manual revisions.

This is a correction to Page 6E3-A3-4 of (Dated 2-11-86) the 1986 Service Manual Volume I.

Note the corrected location of the Fuel Pump Connector "C8" in Figure A3-3. It is located just behind the battery on the left side of the page.

Please correct your 1986 Buick Chassis Service Manual (Volume I).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.