ENGINE LIFTING HOOK ESSENTIAL TOOL J-28467-50. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# ENGINE LIFTING HOOK ESSENTIAL TOOL J-28467-50

#### Models Affected: 1985 Electra With 3.8L (Vin Code 3) Engines

Essential Tool J-28467-50, 3.8L Engine Lifting Hook, was recently shipped. The 3.8L lift hook has a bend in the hook to clear the radiator hose when used with engine support fixture J-28467.

The straight hook in the support fixture package is used on the 4.3L diesel.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.