Body and Accessories. Buick GL7 (Export) 2000

For 1990-2009 cars

# Body and Accessories

## All Component Locator

- Theft Deterrent System Component Views

## All Description and Operation

- Vehicle Theft Deterrent (VTD) Description
- Vehicle Theft Deterrent (VTD) Operation
- Vehicle Theft Deterrent (VTD)Circuit Description

## All Visual Identification

- Theft Deterrent System Connector End Views

## Cleaning, Inspection, and Adjustment

- Programming Additional Keys
- Programming Replacement Keys, Ignition Cylinder, or Powertrain Control Module

## Diagnostic Procedures

- Diagnostic Starting Point - Theft Deterrent
- Diagnostic System Check - Theft Deterrent
- SECURITY Indicator Always On or Flashing
- SECURITY Message Inoperative
- Symptoms - Theft Deterrent

## Diagnostic Trouble Codes

- Diagnostic Trouble Code (DTC) List/Type
- DTC B1009 EEPROM Checksum Error
- DTC B2734 Coded Key Controller Memory Failure
- DTC B2960 Invalid Coded Key Present
- DTC B3031 Key Decoder Device in Assem Learn Mode
- DTC B3055 Key Not Present

## Electrical/Electronic Schematic Diagrams

- Theft Deterrent System Schematics

## General Diagnostic Information

- Scan Tool Data Definitions
- Scan Tool Data List

## Removal, Installation, and Replacement

- PASS-Key III Module Replacement