Keyless Entry System Does Not Change Customization Modes. Buick GL7 (Export) 2000

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Keyless Entry Diagnostic System Check? | -- | Go to Step 2 | Go to Diagnostic System Check - Remote Keyless Entry
2 | Attempt to customize the keyless entry customer options. Refer to Remote Unlock Control Customization . Were you able to change the customer customization? | -- | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems | Go to Step 3
3 | Important: Perform the body control module (BCM) programming procedure when replacing the BCM. Replace the BCM. Refer to Body Control Module Replacement . Did you complete the repair? | -- | System OK | --