Fastener Tightening Specifications. Buick Roadmaster 1996

For 1990-2009 cars

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Coolant Recovery Reservoir Nuts | 6 | -- | 53
Electric Engine Cooling Fan Bolt | 6 | -- | 53
Engine Oil Cooler Fitting Nut | 27 | 20 | --
Fan Blade Bolt | 24 | 18 | --
Fan Blade Clutch Nut | 24 | 18 | --
Knock Sensor | 19 | 14 | --
Negative Battery Cable | 17 | 13 | --
Radiator Air Lower Deflector Bolt | 1.5 | -- | 13
Radiator Air Side Deflector Bolt | 1.9 | -- | 17
Radiator Fan Shroud Screw | 6 | -- | 53
Radiator Upper Fan Shroud Screw | 6 | -- | 53
Radiator Upper Mounting Panel Screw | 6 | -- | 53
Transmission Oil Cooler Fitting Nut | 27 | 20 | --
Coolant Pump Inlet Bolt | 28 | 21 | --