Cooling System Components. Buick Roadmaster 1996

For 1990-2009 cars

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
Engine Cooling Fan Motor (Primary) | Behind the RH side of the radiator | 8A-201-40 Fig 64 | -- | 1.055
Engine Cooling Fan Motor (Secondary) | Behind the LH side of the radiator | 8A-201-40 & 41 Fig 64 & 66 | -- | 1.055
Engine Cooling Fan Relay (Primary) | In U/H electrical center | 8A-201-6 Fig 13 | -- | 1.055
Engine Cooling Fan Relay (Secondary) | In U/H electrical center | 8A-201-6 Fig 13 | -- | 1.055
Powertrain Control Module (PCM) | Engine compartment, forward of the LH wheelhouse, under the air cleaner | 6-Engine Controls | -- | 3.670
C1 (32 cavities) | Engine harness to PCM, forward of the LH wheelhouse, under the air cleaner | -- | 6-Engine Controls | --
Underhood Electrical Center | Engine compartment, attached to the RH wheelhouse | 8A-201-9 Fig 15 | -- | --
C103 (5 cavities) | F/L harness to engine harness, at RH fender | -- | -- | --
C104 (4 cavities) | F/L harness to cooling fans jumper, near the battery | 8A-201-40 Fig 63 | -- | --
G106 | RH headlamp support, forward of the battery | 8A-201-10 Fig 17 | -- | --
S111 | Engine harness, about 15 cm (5.9 in) from U/H electrical center | -- | -- | --