INCORRECT BATTERY INSTALL NEW BATTERY. Buick Roadmaster 1993

For 1990-2009 cars

# INCORRECT BATTERY INSTALL NEW BATTERY

#### Subject: INCORRECT BATTERY

#### Models: 1993 Chevrolet Caprice Police Car

#### TO: ALL GENERAL MOTORS DEALERS:

General Motors of Canada Limited has detemined that certain 1993 Chevrolet Caprice Police Car (SEO 9C1) model vehicles were assembled with batteries which do not meet the specifications advertised in vehicle literature and bid package information. Vehicle literature and bid package information identified a 730 CCA (Cold Cranking Amp) battery, however the involved vehicles were assembled with 690 CCA batteries.

To correct this condition, dealers are to install a new A/C Delco battery with 770 CCA (730 CCA batteries are no longer available), or provide a refund of $35.00 in place of receiving the 770 CCA battery (vehicle owner's option).

#### VEHICLES INVOLVED:

Involved are certain 1993 Chevrolet Caprice Police Car model vehicles within the following VIN breakpoints:

Year Model Plant Plant Code From Through 1993 B-Car Willow Run "W" PW100002 PW115177

All affected vehicles have been identified by the VIN listing provided to involved dealers with this bulletin. Any dealer not receiving a listing was not shipped any of the affected vehicles.

DEALER CAMPAIGN RESPONSIBILITY:

All unsold new vehicles in dealer's possession and subject to this campaign must be held and inspected/repaired per the Service Procedure of this Campaign Bulletin before owners take possession of these vehicles.

Dealers are to perforrm this campaign on all involved vehicles at no charge to owners, regardless of ldlometres traveled, age of vehicle, or ownership, from this time forward.

Owners of vehicles recendy sold from your new vehicle inventory with no owner information indicated on the dealer listing, are to be contacted by the dealer, and arrangements made to make the required coffection according to instructions contained in this bulletin. This could be done by mailing to such owners a copy of the owner letter accompanying this bulletin. Campaign follow-up cards should not be used for this purpose, since the owner may not as yet have received the notification letter.

In summary, whenever a vehicle subject to this campaign is taken into your new or used vehicle inventory, or is in your dealership for service in the future, please take the steps necessary to be sure the campaign correction has been made before selling or releasing the vehicle.

#### CAMPAIGN PROCEDURE:

Refer to Section 4 of the Service Policies and Procedures Manual for the detailed procedure on handling Product Campaigns. Dealers are requested to complete the campaign on all transfers as soon as possible.

#### OWNER NOTIFICATION:

All owners of record at the time of campaign release are shown on the attached computer listing and have been notified by first class mail from General Motors (see copy of owner letter included with this bulletin). The listings provided are for campaign activity only and should not be used for any other purpose.

#### PARTS INFORMATION:

Batteries required to complete this campaign are to be obtained from your local A/C Delco battery supplier.

Part Number Description Quantity/Vehicle

78A72 (A/C Delco P/N) 770 CCA Battery 1

#### NOTICE: Battery cannot be returned to A/C Delco or GMSPO for warranty or parts credit.

PARTS AND LABOR CLAIM INFORMATION:

Credit for the campaign work performed will be paid upon receipt of a properly completed campaign claim card or DCS, transmission in accordance with the following:

Repair Code Description Time Allowance

2A Instll New Battery 0.4 6A Refund Cost Differential in Battery Types *

* 0.2 Hours allowed for refund administration.

Repair Code 2A includes time allowance 0. 1 hour for dealer administrative detail associated with this campaign. Parts credit will be based on dealer net plus 30% to cover parts handling.

#### NOTICE: For either repair code operation, the signed "Option Selection Form" must be attached to the dealer file copy of the repair order.

#### SERVICE PROCEDURE:

FOR ALL INVOLVED VEHICLES

Have owner sign and date "Option Selection Form" (included with the owner notification letter) indicating which option the owner is choosing (refund or battery replacement). Proceed with service procedure which follows ff owner chooses to have battery replaced. If owner instead chooses to receive refund, install Campaign Identification Label and proceed to "Claim Information" section of bulletin.

#### NOTICE: WHEN HANDLING A BATTERY, THE FOLLOWING SAFETY PRECAUTIONS SHOULD BE FOLLOWED:

- Hydrogen gas is produced by the battery. A flame or spark near the battery may cause the ps to ignite.

- Battery (electrolyte) fluid is highly acidic. Avoid spilling on clothing or other fabric. Any spilled electrolyte should be flushed from affected areas with large quantities of water and cleaned immediately.

- Battery should remain in horizontal position to ensure clectrolyte fluid remains over plates. Failure to keep plates covered with electrolyte fluid could cause sparking.

1. Remove 690 CCA battery and install 770 CCA battery following "Battery Assembly Replacement Procedure" on Page 6D1-8 in the 1993 Chevrolet Caprice Service Manual.

2. Destroy 690 CCA battery following procedure below:

a. Place battery on a flat surface. b. Place 13/16" deep well socket over battery cable connector. c. Insert a 4" long bolt (as assembled in illustration on Page 4) into socket and screw into terminal until it bottoms; then back off one turn. d. Turn locknut until terminal connector nut is pulled out of battery.

#### NOTICE: While tuming locknut, bolt head must be held with a wrench and 13/16" deep socket must not rotate.

3. Install Campaign Identification Label.

INSTALLATION OF CAMPAIGN IDENTEFICATION LABEL

Clean surface of radiator upper mounting panel and apply a Campaign Identification Label. Make sure the correct campaign number is inserted on the label. This will indicate that the campaign has been completed.

General Motors of Canada bulletins are intended for use by professional technicians, NOT a "do-it-yourselfer." They are written to inform these technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions, and know-how to do a job properly and safely. If a condition is descrition, DO NOT assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See your General Motors dealer for information on whether your vehicle may benefit from the information.

Dear General Motors Customer

General Motors of Canada Limited has determined that certain 1993 Chevrolet Caprice Police Car model vehicles were assembled with batteries which do not meet the specifications advertised in vehicle literature and bid package information. Vehicle literature and bid package information identified a 730 CCA (Cold Cranking Amp) battery, however the involved vehicles were assembled with 690 CCA batteries.

To correct this condition, General Motors is offering you a choice of the following:

A. Have a new battery with 770 CCA (730 CCA batteries are no longer available) installed at no charge to you.

B. Receive a refund of $35.00 in place of receiving a new battery.

Please contact your GM dealer as soon as possible to arrange a service date or arrange to receive the refund. Also, complete and sign the enclosed Option Selection Form and present it to your dealer as notification of your choice. Instructions for making this correction have been sent to your dealer. If you wish to receive the new battery, please ask your dealer how much time will be needed to schedule and process your vehicle.

This letter identifies your vehicle. Presentation of this letter to your dealer will assist their Service personnel in completing the necessary correction to your vehicle in the shortest possible time.

We are sorry to cause you this inconvenience; however, we have taken this action in the interest of your continued satisfaction with our products.

Customer Support Department General Motors of Canada Limited

OPTION SELECTION FORM

As owner of a 1993 Chevrolet Caprice involved in Campaign 3N05 (Vehicle Identirication Number I select:

Option A - New Battery Installation

OR

Option B - $35.00 Refund

Owner Signature Date

NOTICE TO DEALERS

For either repair code operation, the signed "Option Selection Form" must be attached to the dealer file copy of the repair order.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.