INTERMITTENT OPERATION OF DECK LID OR BACK GLASS WITH REMOTE. Buick Roadmaster 1992

For 1990-2009 cars

# INTERMITTENT OPERATION OF DECK LID OR BACK GLASS WITH REMOTE

APPLICATION: 1992 B-CAR (BUICK ONLY)

#### CONDITION:

THE DECK LID OR THE REAR BACK WINDOW GLASS MAY OPERATE INTERMITTENTLY ON THE 1992 B-CAR, IN VEHICLES WITH THE REMOTE KEYLESS ENTRY (RKE) OPTION (RPO AU0).

#### CORRECTION:

A NEW RKE RECEIVER, P/N 10220991, WAS RELEASED FOR PRODUCTION EFFECTIVE WITH VIN BREAKPOINTS NR463050 ON SEDANS, AND NW408644 ON WAGONS.

REPLACE THE RECEIVER, AS SHOWN IN SECTION 9K OF THE SERVICE MANUAL.

#### PART AVAILABILITY:

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

LABOR OPERATION: R4480

LABOR TIME: 0.8 HR. SEDAN 0.9 HR. WAGON

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1992 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.