SEALING MATERIALS FOR OIL LEAKS. Buick Skyhawk 1987

For 1990-2009 cars

# SEALING MATERIALS FOR OIL LEAKS

#### VEHICLES AFFECTED: 1987 LL8 2.0L OHV (VIN CODE 1) ENGINE IN 'J' AND 'L' VEHICLES

Warranty repair information is indicating that rocker cover, cam cover, and front timing cover leakage repairs are being made with RTV. RTV should not be used on these applications.

These sealing interfaces have been designed only for the specified gaskets as follows:

Rocker Cover Gasket P/N 14090066

Cam Cover Gasket P/N 14090974

Front Timing Cover Gasket P/N 14090026

Use of any other material will not meet the intended sealing life.

This service bulletin is for information only.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.