ELECTRICAL TROUBLESHOOTING MANUAL CORRECTIONS. Buick Skyhawk 1985

For 1990-2009 cars

# ELECTRICAL TROUBLESHOOTING MANUAL CORRECTIONS

#### VEHICLES AFFECTED: 1985 All Series

The 1985 Oldsmobile Electrical Troubleshooting Manual Supplement - All Series requires the following corrections.

Firenza section page 22-3, shows the fuel pump relay normally closed from Terminal 'A' to Terminal 'E'. The relay should be normally closed from Terminal 'A' to Terminal 'D'.

#### NOTE: IN REPAIRING A VEHICLE, THE TECHNICIAN MAY HAVE TO REFER TO THE ETM SUPPLEMENT WHICH CONTAINS RUNNING PRODUCTION CHANGES AND CORRECTIONS.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.