LOOSE HEADLINER RETAIN STRIPS SECURE STRIPS WITH SCREWS. Buick Skyhawk 1982

For 1990-2009 cars

# LOOSE HEADLINER RETAIN STRIPS SECURE STRIPS WITH SCREWS

Skyhawk hook and loop headliner retaining strips are retained to roof sheet metal reinforcements with screws in 1983 and late 1982. If adhesive bond does not hold fastener on earlier Skyhawks, secure retaining strips with screws.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.