INNER TIE ROD TO GEAR BOLT LOCK PLATE REPLACEMENT. Buick Skyhawk 1985

For 1990-2009 cars

# INNER TIE ROD TO GEAR BOLT LOCK PLATE REPLACEMENT

#### Models Affected: 1985 Skyhwak and Somerset Regal

The inner tie rod bolt lock plate has been changed from the tab type lock plate to a push on retainer type lock plate on 1985 Skyhawk and Somerset Regal models.

The new push on lock plate, part no. 7836778 must be replaced with a new one any time it is removed. Replacement is necessary as the plate may be damaged during removal and may not retain properly if reused. See illustration.

The new lock plate will be include with future packages of tie rods and center take-off short gears.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.