1989 NEW VEHICLE ANNOUNCEMENT PAINT CODES-WARRANTY INFO.. Buick Skyhawk 1989

For 1990-2009 cars

# 1989 NEW VEHICLE ANNOUNCEMENT PAINT CODES-WARRANTY INFO.

#### MODELS AFFECTED: ALL 1989 BUICKS

1. 1989 Warranty and Owner Assistance Information Booklets

2. 1989 Buick Service Manuals

3. 1989 Buick Owner's Manuals

4. 1989 Vehicle Certification and Tire Pressure Label

5. 1989 Service Parts Identification Label

6. 1989 New Vehicle Inspection Procedure Sheets

7. 1989 Buick Passenger Car Maintenance Schedule Booklet

8. 1989 Buick Labor Time Guide

9. 1989 Buick Bulletin Binders

10. 1989 Paint Codes

1. WARRANTY AND OWNER ASSISTANCE ON 1989 BUICK NEW CARS ---------------------------------------------------- For 1989, a single booklet containing warranty information relative to the new car, emission systems, tire and corrosion is used:

#25532249 - 1989 Warranty and Owner Assistance Information For Buick New Cars

Owner assistance satisfaction procedures, the GM mediation/arbitration program, special policy adjustment programs, and the GM Protection Plan are all outlined in this booklet. A separate tire warranty folder is included to outline warranty as provided by individual tire manufacturers.

The owner's name, address, Vehicle Identification Number, date of delivery and mileage at the time of delivery, are all to be typed on the inside of the front cover of the booklet in the space provided. There is a space provided on the back of the folder for the dealer name, address and dealer code.

It is very important that the Owner and Vehicle Information on the booklet be correct. This information will be the only means of owner identification for repairs covered under warranty. In order for dealer warranty claims to be properly processed, the Vehicle Identification Number must be correct. Owners should be instructed to carry their Warranty and Owner Assistance Information booklets in their vehicles at all times.

2. 1989 SERVICE MANUALS --------------------- 1989 service manuals will be shipped to all Buick dealers in September 1988, as follows:

- LeSabre & Electra/Park Avenue New Product Tnformation Chassis Manual - LeSabre & Electra/Park Avenue New Product Information Electrical Systems Manual - LeSabre & Electra/Park Avenue Body Service Manual - Riviera/Reatta New Product Information Manual - Skyhawk & Skylark New Product Information Manual - Century Service Manual - LeSabre & Electra Estate Wagons Service Manual - Regal Service Manual

Final edition manuals, which replace New Product Information manuals, where applicable, will be published & shipped to all Buick dealers in early 1989.

Beginning with the 1989 LeSabre & Electra/Park Avenue New Product Information Electrical Systems Manual, the Buick LeSabre & Electra/Park Avenue will have a specifically designed service manual for electrical systems. The electronic & electrical complexity of these cars has been addressed with inclusive accurate information that is heavily illustrated to eliminate much of the normal text. This manual provides complete service information for each electrical system & is exclusive to Buick for 1989. Other features include:

- Electrical schematics with point-to-point checks & component operation included. - Complete electrical harness & component location illustrations. - Illustrated remove, repair & install procedures. - Diagnosis tables or "trouble tree" charts. - Service part name reference chart.

Similarly, the Buick LeSabre & Electra/Park Avenue will have a specifically designed Body Service Manual which includes heavily illustrated Remove, Repair, Install & Adjust procedures. Much of the normal text is replaced by these illustrations.

Additional manuals can be ordered on the "Service Publications for Buick Dealers" order form which is included, with the manual shipments or available from your Zone/Branch Office.

3. 1989 OWNER'S MANUALS -------------------- For 1989 there are a total of nine (9) owner's manuals.

Part # 25532259 - Century Part # 25533510 - LeSabre & Electra Estate Wagons Part # 25532243 - Electra/Park Avenue Part # 25533511 - Riviera Part # 25533514 - Regal Part # 25532247 - LeSabre Part # 25533512 - Skyhawk Part # 25533513 - Skylark Part # 25533515 - Reatta

4. 1989 VEHICLE CERTIFICATION AND TIRE PRESSURE LABEL -------------------------------------------------- In accordance with Federal Motor Vehicle Regulations, A Vehicle Certification and Tire Pressure Label is being affixed to all 1989 model Buicks.

The label will have a certification statement, Vehicle Identification Number, month and year that the vehicle was built. The label will be attached horizontally to the left front door inner panel lock facing on all models.

The lower portion of the label will have the tire size and tire pressure information.

Due to the certification label's location, it may be subject to damage during car shipment and new vehicle pre-delivery service or may be required due to door repair or replacement.

To acquire a replacement certitication label, proceed as follows:

A. Check Vehicle Identification Number on engine block and identification number on instrument panel to see that they match.

B. Send a readable machine copy of the vehicle invoice, along with a letter of explanation to your Zone/Branch Office, Attention Ass't. Zone Manager

- Service/Branch Manager.

5. SERVICE PARTS IDENTIFICATION LABEL ---------------------------------- Assembly centers no longer use a Body Number Plate that contains paint and trim information. This information, along with options and build content is now recorded on the Service Parts Identification (SPID) label. Care should be taken to transfer the SPID label or its information, if panel to which label is affixed requires replacement. Replacement SPTD labels are not available.

6. 1989 NEW VEHICLE INSPECTION PROCEDURE FORM ------------------------------------------ For the New Vehicle Inspection and Delivery Procedure which was introduced in 1983, use New Vehicle Inspection Procedure Sheet 101072, revised 8/88. This form is shipped with each Buick delivered to you. Additional forms may be obtained through your Publication Service Order Form.

7. 1989 MAINTENANCE SCHEDULE ------------------------- For 1989 there is one (1) vehicle maintenance schedule booklet for all cars, part number 10077730.

8. 1989 LABOR TIME GUIDE - MICROPUBLICATIONS UPDATE AND REQUEST FOR REVIEW FORMS ----------------------------------------------------------------------- Approximately September, 1988, one (1) set of micropublications will be mailed to all dealers, each set will consist of the following material:

- Labor Time Guide - Dealer Service Bulletin Update - Dealer Campaign Bulletin Update - 1988 Service Manuals

Additional quantities, if previously ordered, will be supplied, based upon records on file at time of mailing. All requests for additional microfiche sets are to be processed directly thru GM Photographic. Additional order forms are available from your Zone Office.

Labor Time Guide - All claims processed on the date of receipt or after will be processed on the basis of operations and labor time allowances provided.

#### Printed Labor Time Guide

The 1989 Labor Time Guide is available in printed format. This loose leaf publication can be ordered on the "Service Publications For Buick Dealers" Order Form. Binders are also available. Printed Labor Time Guides will automatically be sent to dealers who have previously ordered on a continuing basis.

9. 1989 BUICK BULLETIN BINDERS --------------------------- Binders and index tabs should be ordered using the "Service Publications For Buick Dealers" Order Form. Binders and tabs have been sent to dealers who previously ordered on a continuing basis.

10. 1989 PAINT CODES ---------------- Color chip sheets for the 1989 Buick Paints will again be available from DuPont, Ditzler, Inmont (Rinshed-Mason), Sherwin Williams, Acme/Rogers and Martin-Senour.

The following charts indicate 1989 exterior paint supplier stock number, the WA numbers and vehicles the paint is used on. The paint numbers listed in this bulletin along with clearcoat materials, are or soon will be available from local paint suppliers. Please note that the Service Parts Identification Label includes paint information.

When contacting your local paint supplier for repair materials, make sure that you specify the type of material needed. If your paint supplier is unable to provide you with the material needed, ask him to contact his manufacturer sales representative for assistance.

#### 1989 BUICK EXTERIOR COLORS

INMONT/ PAINT SERIES PPG RINSHED CODE COLOR WA# USAGE DITZLER DUPONT MASON ---- ----- --- ----- ------- ------ ----- 11 WHITE C/O 3967 ABJ 2058 5338 2080

12 SILVER MET C/O 8535 AJ 3746 B8501 15001 15 MED. GRAY MET. C/O 8573 ABJ 3749 B8502 15004

9000/ A946 19 BLACK C/O 848 AB 9300 99S PKG EP403 M403

** 26 LT. BLUE MET. C/O 8964 ABJ 3966 B8704 17005

** 29 DK. MED. BLUE C/O 8970 AB 3968 B8706 17007

52 COPPER BEIGE B/C 8973 B 4088 B8710 18OU7 57 LT. BEECHWOOD MET. 9180 ABJ 4090 B8872 18008 59 DK. BEECHWOOD MET. 9181 AB 4092 B8875 18009 70 CARMINE 8530 J 3781 B8512 15035 75 MED. GARNET RED MET. 8980 AB 3988 B8715 17022 79 DK. RED MET. 8529 B 3786 B8509 15040

PAINT SERIES SHERWIN-WILLIAMS MARTIN CODE COLOR WA# USAGE (ACME-ROGERS) SENOUR ---- ----- --- ----- ------------- ------ LIOA-2864 11 WHITE C/O 3967 ABJ 5644 (ACME) 5644 (ROGERS) 30-3929 12 SILVER MET C/O 8535 AJ 34380 30-5371 15 MED. GRAY MET. C/O 8573 ABJ 34381 30-3572

LIOB-1738 19 BLACK C/O 848 AB 3000 (ACME) 3069 4590 (ROGERS)

** 26 LT. BLUE MET. C/O 8964 ABJ 35865 35865

** 29 DK. MED. BLUE C/O 8970 AB 35866 35866

52 COPPER BEIGE B/C 8973 B 37082 37082 57 LT. BEECHWOOD MET. 9180 ABJ 37084 37084 59 DK. BEECHWOOD MET. 9181 AB 37086 37086 70 CARMINE 8530 J 34401 30-5392 75 MED. GARNET RED MET. 8980 AB 35871 35871 79 DK. RED MET. 8529 B 34405 30-5396

#### 1989 BUICK EXTERIOR COLORS

INNONT/ PAINT SERIES PPG RINSHED CODE COLOR WA# USAGE DITZLER DUPONT MASON ---- ----- --- ----- ------- ------ ----- 78 MED. ROSEWOOD MET. C/O 8986 A 3991 B8717 17024 40 WHITE C/C C/O 8554 NWHCE33 3680 B8469 13570 13 SILVER MET C/C C/O 9021 NWHCE33 3822 D8590 15365 87 GUN METAL MET C/C 9243 NWHCE33 4009 B8729 17038 41 BLACK C/C C/O 8555 HC33 9700 99S 13572 14 BLACK MET. C/O 8767 NEW 3961 8701 17002 22 LT. BLUE MET. B/C C/O 8966 NWHE 3964 B8703 17003 28 BLACK SAPPHIRE MET. B/C C/O 8743 HCE 3885 B8618 16003 83 MED. BLUE FM MET. B/C C/O 8993 CE33 3995 B8720 17028 27 MED. BLUE MET B/C C/O 8742 NW 3967 B8705 17004 62 LT. BEECHWOOD MET B/C 9089 NWH 4094 B8877 18003 69 MED. BEECHWOOD MET B/C 9091 H 4109 B8880 18004 51 COPPER BEIGE B/C C/O 89/3 NW 3976 B8710 17014 67 DK. ANTELOPE MET. B/C 9094 CE 4096 B8879 18006 86 ANTELOPE BEIGE B/C 92OU C 4101 B8886 18015 95 LT. ANTELOPE F/M B/C 9093 CE 4104 B8889 18005 72 MED. GARNET RED MET. * B/C C/O 8979 CENWH 3986 B8713 17021 76 DK. GARNET MED MET. * B/C C/O 8984 CENH33 3989 B8716 17023 73 BRILLIANT RED B/C 9348 W 4098 B8881 18014 81 BRIGHT RED C/O 8774 33 3794 C8508 15265 80 LT. ROSEWOOD MET. B/C C/O 8992 E 3993 B8718 17027 82 MED. ROSEWOOD MET. * B/C C/O 8990 E 3994 B8719 17026

PAINT SERIES SHERWIN-WILLIAMS MARTIN CODE COLOR WA# USAGE (ACME-ROGERS) SENOUR ---- ----- --- ----- --------------- ------ 78 MED. ROSEWOOD MET. C/O 8986 A 35873 35873 40 WHITE C/C C/O 8554 NWHCE33 33755 30-5295 13 SILVER MET C/C C/O 9021 NWHCE33 35369 30-5491 87 GUN METAL MET C/C 9243 NWHCE33 36724 36724 41 BLACK C/C C/O 8555 HC33 33756 30-5296 14 BLACK MET. C/O 8767 NEW 3587/ 35877 22 LT. BLUE MET. B/C C/O 8966 NWHE 35879 35879 28 BLACK SAPPHIRE MET. B/C C/O 8743 HCE 35313 30-5520 83 MED. BLUE FM MET. B/C C/O 8993 CE33 35900 35900 27 MED. BLUE MET B/C C/O 8742 NW 35882 35882 62 LT. BEECHWOOD MET B/C 9089 NWH 37088 37088 69 MED. BEECHWOOD MET B/C 9091 H 37091 37091 51 COPPER BEIGE B/C C/O 89/3 NW 35887 35887 67 DK. ANTELOPE MET. B/C 9094 CE 37090 37090 86 ANTELOPE BEIGE B/C 92OU C 37091 37097 95 LT. ANTELOPE F/M B/C 9093 CE 37099 37099 72 MED. GARNET RED MET. * B/C C/O 8979 CENWH 35894 35894 76 DK. GARNET MED MET. * B/C C/O 8984 CENH33 35895 35895 73 BRILLIANT RED B/C 9348 W 3/093 37093 81 BRIGHT RED C/O 8774 33 34983 30-5464 80 LT. ROSEWOOD MET. B/C C/O 8992 E 35898 35898 82 MED. ROSEWOOD MET. * B/C C/O 8990 E 35896 35896

B/C - BASECOAT/CLEARCOAT C/O - CARRY OVER COLOR * - NEW ON THIS CAR LINE

#### 1989 BUICK STRIPING COLORS

INMONT/ PAINT PPG RINSHED CODE COLOR WA# DITZLER DUPONT MASON ---- ----- --- ------- ------ ------ 11A WHITE C/O 396/ 2058 5338 2080 14A LT. GRAY 8670 33856 C8529 18A GUN METAL C/O 8291 33750 C8441 14036

19A BLACK C/O 848 9300 99S A946 20A LT. SAPPHIRE C/O 7456 16319 D8009 21A DK. SAPPHIRE 9103 16313 C8787 17055 34A MED. BEECHWOOD 9274 26298 D8869 49A ANTELOPE BEIGE 9200 4101 B8886 55A GOLD C/O 8589 25509 D8276 150/6G 59A COPPER BEIGE 8973 25894 D8753

66A ORANGE 8002 60909 45261

67A DK. BROWN C/O 8001 25088 45260 9502 68A LT. ROSEWOOD 8874 51283 C8782 /2A DK. ROSEWOOD 8872 51282 C8783 17050 /3A DK. GARNET 9106 51286 C8790

75A RED C/O 4721 72128 43592 4518R 76A GARNET RED 8852 51211 C8643 79A DK. GARNET 8863 51167 C8525

PAINT SHERWIN-WILLIAMS MARTIN CODE COLOR WA# (ACME-ROGERS) SENOUR ---- ----- --- ------------- ------ 11A WHITE C/O 396/ L10A-2864 14A LT. GRAY 8670 5644 (ACME) 18A GUN METAL C/O 8291 5644 (ROGERS) 32-3929 34869 26729 34102 26700 19A BLACK C/O 848 L1OB-1738 20A LT. SAPPHIRE C/O 7456 3000 (ACME) 21A DK. SAPPHIRE 9103 4590 (ROGERS) 3069 34A MED. BEECHWOOD 9274 36466 36466 49A ANTELOPE BEIGE 9200 36464 36464 55A GOLD C/O 8589 38403 38403 59A COPPER BEIGE 8973 38402 38402 34105 26703 36402 36462 66A ORANGE 8002 J4-8728 25455 (ACME) 25455 (ROGERS) 26337 67A DK. BROWN C/O 8001 J4-8728 68A LT. ROSEWOOD 8874 25455 (ACME) /2A DK. ROSEWOOD 8872 25455 (ROGERS) 26336 /3A DK. GARNET 9106 36460 36460 36459 36459 36465 36465 75A RED C/O 4721 J4-7191 76A GARNET RED 8852 11892 (ACME) 79A DK. GARNET 8863 11892 (ROGERS) 26272 35566 26780 34868 26728

#### 1989 BUICK VINYL ROOF COLORS

INMONT/ PAINT SERIES PPG RINSHED CODE COLOR WA# USAGE DITZLER DUPONT MASON ---- ----- --- ----- ------- ------ ----- 2-1094 11T WHITE C/O 8936 ACHE 2-130 B8469 16110

19T BLACK C/O 848 ACH -120 B8479 4416

28T BLACK SAPPHIRE MET. C/O 8743 CHE 2-1273 B8618

62T LT. BEECHWOOD MET. 9089 2-1314 B8877 76T DK. GARNET RED MET. C/O 8984 CHE 2-1272 B8716 79T DK. RED MET. C/O 8529 A 2-1105 B8509 15187F 82T MED ROSEWOOD MET. 8990 C 2-1266 B8719 84T GUNMETAL MET. C/O 7782 ACHE 2-1053 B8403 14040 86T LT. ANTELOPE 9200 C 2-1300 B8886 72T MED. GARNET RED 8979 CH*E 2-1268 B8713 29T DK. SAPPHIRE BLUE IND. 8970 A 2-1295 B8706 17079 57T LT. BEECHWOOD IND. 9180 A 2-1297 B8872 18073 78T MED. ROSEWOOD IND. 8986 A 2-1317 B8717 18077 13T SILVER 7781 HE 2-1052 B8402 22T LT. BLUE 8966 HE 2-1271 B8703 85T LT. ROSEWOOD 8992 E 2-1285 B8718 95T LT. ANTELOPE MET. 9093 E 2-1301 B8889 93* WHITE DIAMOND MET 8933 E BASE FOR 4175 GROUND COAT PPG 3680 INTERMEDIATE TOP FOR 3680 COAT PPG 4175

PAINT SERIES SHERWIN-WILLIAMS MARTIN CODE COLOR WA# USAGE (ACME-ROGERS) SENOUR ---- ----- --- ----- ---------------- ------ 11T WHITE C/O 8936 ACHE 35781 26851 J4-1990 19T BLACK C/O 848 ACH 9739 (ACME) 16082 9739 (ROGERS) 28T BLACK SAPPHIRE MET. C/O 8743 CHE 36593 36593

62T LT. BEECHWOOD MET. 9089 38561 38561 76T DK. GARNET RED MET. C/O 8984 CHE 36597 36597 79T DK. RED MET. C/O 8529 A 35086 26760 82T MED ROSEWOOD MET. 8990 C 36598 36598 84T GUNMETAL MET. C/O 7782 ACHE 34124 26705 86T LT. ANTELOPE 9200 C 38567 38567 72T MED. GARNET RED 8979 CH*E 36596 36596 29T DK. SAPPHIRE BLUE IND. 8970 A 37032 37032 57T LT. BEECHWOOD IND. 9180 A 38566 38566 78T MED. ROSEWOOD IND. 8986 A 38560 38560 13T SILVER 7781 HE 34123 26704 22T LT. BLUE 8966 HE 36595 36595 85T LT. ROSEWOOD 8992 E 36599 36599 95T LT. ANTELOPE MET. 9093 E 38563 38563 93* WHITE DIAMOND MET 8933 E 39244 39244 39245 39245

C/O - CARRY OVER COLOR * - NEW ON THIS CAR LINE

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.