TRANSAXLE CONVERTER COVER INTERFERENCE NOISE - REPAIR. Buick Skyhawk 1985

For 1990-2009 cars

# TRANSAXLE CONVERTER COVER INTERFERENCE NOISE - REPAIR

#### MODELS AFFECTED: 1985-86 SKYHAWKS EQUIPPED WITH 2.0L ENGINES (VIN CODE P)

Some 1985 and early 1986 Skyhawks cars with automatic transaxles may exhibit a noise generated by an interference condition between the plastic transaxle converter cover and the flexplate.

Vehicles exhibiting this condition may be repaired by replacing the plastic converter cover with a new one part #14094881.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.